**STEINEL Professional Presence detector**

**IR Quattro SLIM**

**DIM**

Type: Presence detector; Dimensions (L x W x H): 55 x 77 x 77 mm; Mains power supply: 120 – 250 V / 50 – 60 Hz; Power supply, detail: 500 VA max., 120 V; Sensor Technology: passive infrared; Application, place: Indoors; Application, place, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Installation site: ceiling; Installation: Installation; Switching zones: 260 switching zones; Electronic scalability: No; Mechanical scalability: No; Mounting height: 2,50 – 4,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Reach, detail: Retina lens and hexagonal Fresnel structure; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 4 x 4 m (16 m²); Reach, presence: 4 x 4 m (16 m²); Twilight setting TEACH: Yes; Twilight setting: 100 – 1000 lx; Time setting: 30 s – 30 min; Switching output 1, resistive: 2000 W; Number of electronic ballasts, DIM interface: 50; Constant-lighting control: Yes; Basic light level function: Yes; Functions: Normal / test mode, Semi-/fully automatic, Pushbutton / switch mode, Manual ON / ON-OFF, Constant-lighting control ON-OFF; Settings via: Remote control, Smart Remote; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave, Master/master; IP-rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: DIM; PU1, EAN: 4007841593612

**Manufacturer** Steinel

**Prod. No.** 593612

**Ordering designation**

Deliver, install and set ready for operation