**STEINEL Professional Photo-cell controller**

**NightMatic 5000-3**

**COM1 - black**

Type: Photo-cell controller; Dimensions (L x W x H): 42 x 95 x 95 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Sensor Technology: Light sensor; Application, place: Outdoors, Indoors; Installation site: wall, corner; Installation: Surface wiring; Twilight setting TEACH: Yes; Twilight setting: 2 – 1000 lx; Output: 2000 W; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.; Fluorescent lamps, electronic ballast: 1500 W; Fluorescent lamps, uncorrected: 1000 VA; Fluorescent lamps, series-corrected: 400 VA; Fluorescent lamps, parallel-corrected: 400 VA; Switching output 1, low-voltage halogen lamps: 2000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 300 W; LED lamps > 8 W: 600 W; Capacitive load in μF: 176 µF; Constant-lighting control: No; Basic light level function: No; Functions: Night economy mode, light ON / OFF in the morning; Settings via: Remote control, Potentiometers, Smart Remote; Interconnection: Yes; Type of interconnection: Master/master; IP-rating: IP54; Material: Plastic; Ambient temperature: -20 – 50 °C; Application, room: outdoors; Colour: black; Colour, RAL: 9005; Manufacturer's Warranty: 5 years; Version: COM1 - black; PU1, EAN: 4007841011680

**Manufacturer** Steinel

**Prod. No.** 011680

**Ordering designation**

Deliver, install and set ready for operation