**STEINEL Professional Multisensor**

**Multisensor Aerosol KNX**

**V3.0**

Type: Other; Dimensions (L x W x H): 33 x 123 x 123 mm; Mains power supply: 30 V; Power consumption: 0,5 W; Power supply, detail: KNX bus; Sensor Technology: Multisensor; Application, place: Indoors; Installation site: ceiling; Installation: Concealed wiring; Twilight setting TEACH: Yes; Twilight setting: 2 – 1000 lx; Constant-lighting control: No; KNX functions: Risk of infection, Udes air, Comfort, CO2, Light level, HVAC output, Logic gate, Air pressure, Humidity output, Day / night function, Dewpoint, Temperature output, VOC; With bus coupling: Yes; Settings via: ETS software, Bluetooth, Bus; With remote control: No; Interconnection: Yes; IP-rating: IP20; Material: Plastic; Ambient temperature: 0 – 40 °C; Application, room: classroom, lecture hall, one-person office, recreation room, duty room, conference room / meeting room, Indoors, kitchenette; Colour: white; Colour, RAL: 9003; Manufacturer's Warranty: 5 years; PU1, EAN: 4007841079192

**Manufacturer** Steinel

**Prod. No.** 079192

**Ordering designation**

Deliver, install and set ready for operation