**STEINEL Professional LED indoor light without sensor**

**RS PRO LED P1 SL**

**warm white V3**

Dimensions (Ø x H): 280 x 110 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Output: 9 W; Luminous flux: 960 lm; Colour temperature: 3000 K; Colour variation LED: SDCM3; Colour Rendering Index CRI: 80-89; With lamp: Yes, STEINEL LED system; Lamp: LED cannot be replaced; LED life expectancy (max. °C): 50000 h; Drop in luminous flux in accordance with LM80: L80B10; Base: without; LED cooling system: Passive Thermo Control; With motion detector: No; Photo-cell controller: No; Basic light level function: No; Soft light start: Yes; Impact resistance: IK03; IP-rating: IP54; Protection class: II; Ambient temperature: 10 – 40 °C; Housing material: Plastic; Cover material: Plastic, opal; Manufacturer's Warranty: 5 years; With remote control: No; Installation site: wall, ceiling; Version: warm white; PU1, EAN: 4007841056056

**Manufacturer** Steinel

**Prod. No.** 056056

**Ordering designation**

Deliver, install and set ready for operation