**STEINEL Professional Presence detector**

**Hallway**

**BT IPD (Slave) - surface**

Type: Presence detector; Dimensions (L x W x H): 62 x 123 x 123 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Sensor Technology: High frequency; Application, place: Indoors; Installation site: ceiling; Installation: Surface wiring; Mounting height: 2,00 – 4,00 m; Reach, radial: 25 x 3 m (75 m²); Reach, tangential: 25 x 3 m (75 m²); HF-system: 5,8 GHz; Detection angle: 360 °; Angle of aperture: 140 °; Optimum mounting height: 2,8 m; Mechanical scalability: No; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Detection: also through glass, wood and stud walls; Twilight setting TEACH: No; Constant-lighting control: No; Basic light level function: No; Settings via: Bluetooth; With remote control: No; Interconnection: Yes; Type of interconnection: Master/slave; Material: Plastic; Ambient temperature: -20 – 50 °C; Application, room: Indoors, corridor / aisle; Colour: white; Colour, RAL: 9010; Manufacturer's Warranty: 5 years; Version: BT IPD (Slave) - surface; PU1, EAN: 4007841064563

**Manufacturer** Steinel

**Prod. No.** 064563

**Ordering designation**

Deliver, install and set ready for operation