**STEINEL Professional Photo-cell controller**

**Light Sensor Dual**

**KNX - concealed, sq. V3**

Type: Constant-lighting controller; Dimensions (L x W x H): 51 x 94 x 94 mm; Power supply, detail: KNX bus; Sensor Technology: Light sensor; Application, place: Outdoors, Indoors; Installation site: wall, ceiling; Installation: Concealed wiring; Mounting height: 2,00 – 4,00 m; Twilight setting TEACH: Yes; Twilight setting: 2 – 1000 lx; Constant-lighting control: Yes; Basic light level function: Yes; KNX functions: Light output 2x, Light level, Constant-lighting control, Photo-cell controller, Logic gate; With bus coupling: Yes; Settings via: ETS software, Remote control, Bus, Smart Remote; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; IP-rating: IP20; Ambient temperature: -20 – 50 °C; Application, room: classroom, one-person office, open-plan office, high-bay warehouse, conference room / meeting room, Indoors; Colour: white; Colour, RAL: 9003; Manufacturer's Warranty: 5 years; Version: KNX - concealed, sq.; PU1, EAN: 4007841058326

**Manufacturer** Steinel

**Prod. No.** 058326

**Ordering designation**

Deliver, install and set ready for operation