**STEINEL Professional Sensor-switched LED floodlight**

**XLED PRO Wide**

**black**

Dimensions (L x W x H): 126 x 265 x 188 mm; Mains power supply: 220 – 240 V / 50 – 60 Hz; Mounting height max.: 6,00 m; Sensor Technology: passive infrared; Output: 24,8 W; Interconnection: Yes; Type of interconnection: Sensor/slave; Interconnection, number: maximum of 10 floodlights; Luminous flux: 2400 lm; Colour temperature: 4000 K; Colour variation LED: SDCM3; Colour Rendering Index: 80-89; With lamp: Yes, STEINEL LED system; Lamp: LED cannot be replaced; LED life expectancy (max. °C): 50000 h; Drop in luminous flux in accordance with LM80: L70B10; LED cooling system: Passive Thermo Control; With motion detector: Yes; Detection angle: 240 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Reach, radial: r = 3 m (19 m²); Reach, tangential: r = 12 m (302 m²); Photo-cell controller: Yes; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Basic light level function time: 10 min, 30 min, all night; Main light adjustable: No; Settings via: Remote control, Potentiometers, Smart Remote; Soft light start: No; Continuous light: selectable, 4h; Impact resistance: IK03; IP-rating: IP54; Protection class: I; Ambient temperature: -20 – 40 °C; Housing material: Aluminium; Cover material: Plastic, transparent; Manufacturer's Warranty: 5 years; Includes corner wall mount: No; PU1, net weight: 1,841 kg; Version: black; PU1, EAN: 4007841010096

**Manufacturer** Steinel

**Prod. No.** 010096

**Ordering designation**

Deliver, install and set ready for operation